**Truepress JET 520HD mono**

The Truepress JET 520HD mono delivers exceptional monochrome printing at a speed up to 150 meters per minute on offset coated or uncoated paper. Ideal for publishing and transactional applications, this high-speed roll-fed digital inkjet press captures small type and barcodes with a precision that is hard to match. The Truepress JET 520HD mono offers 1,200 x 1,200 dpi resolution using water-based inks cured with a near-infrared dryer. Your transition to finishing will be seamless with this press.

**Truepress JET 520HD mono Highlights**

* Resolution of 1,200 x 1,200 dpi
* Speed up to 150 meters per minute
* Accepts coated and uncoated paper
* NIR dryer
* Water-based ink