**Truepress JET 520NX**

Single-pass “white paper factory” printing has never been easier with the Truepress JET 520NX. Without the need to preprint shells, direct mail, commercial and transactional printers can exceed their clients’ expectations with variable data capabilities available in full-color or monochrome options on uncoated paper. Printing at a resolution of 600 x 900 dpi, the Truepress JET 520NX reaches speeds up to 150 meters per minute with CMYK formulas and 180 meters per minute as a monochrome press complemented with a black enhanced option. This press is designed for maximum uptime and the lowest cost of ownership available in continuous feed inkjet printing. Available in straight or L shape configurations, the Truepress JET 520NX is the ideal machine for the compact pressroom.

**Truepress JET 520NX Highlights**

* Flexible configurations
* Speed up to 180\* meters per minute
* 600 x 900 dpi resolution
* Accommodates uncoated stock
* Black enhanced option\*

\*Monochrome model