**Truepress PAC 830F**

The Truepress PAC 830F is a high-speed, water-based inkjet press specifically designed for the flexible packaging industry. Using drop-on-demand inkjet technology, it can handle film or plastic up to 830 millimeters wide at an industry-leading speed of 75 meters per minute. The system prints a resolution of 1,200 x 1,200 dpi using a built-in primer coater that increases ink adherence. Its CMYK and white aqueous inks conform to food safety regulations, making it an ideal choice for packaging printers looking to reach multiple markets.

**Truepress PAC 830F Highlights**

* Resolution of 1,200 x 1,200 dpi
* Accommodates PET and OPP substrates
* Speed up to 75 meters per minute
* Food-safety compliant
* CMWK+W aqueous inks